<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<packages>
<package name="SIL-16">
</package>
<package name="2X8">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="DIL28-3">
<description>&lt;TABLE CELLSPACING=1 CELLPADDING=2&gt;
&lt;TR BGCOLOR=#0066FF&gt;&lt;TD COLSPAN=2 ALIGN=CENTER&gt;&lt;FONT COLOR=#FFFFFF&gt;&lt;B&gt;Specifications&lt;/B&gt;&lt;/FONT&gt;&lt;/TD&gt;&lt;/TR&gt;
&lt;TR BGCOLOR=#999999&gt;&lt;TD &gt;&lt;B&gt;Parameter&lt;/B&gt;&lt;/TD&gt;&lt;TD&gt;&lt;B&gt;Value&lt;/B&gt;&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD&gt;Type of Package &lt;/TD&gt;&lt;TD&gt;DIL (Dual in Line)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD&gt;Amount of Pins&lt;/TD&gt;&lt;TD&gt;28&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD&gt;Dimensions&lt;/TD&gt;&lt;TD&gt; 34.6 x 7.3 mm&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD&gt;Pitch&lt;/TD&gt;&lt;TD&gt; 2.54 mm&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="16FPC-V">
<description>&lt;b&gt;1mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
<package name="16FPC-H">
<description>&lt;b&gt;1mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
<package name="14FPC-H">
<description>&lt;b&gt;1mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
<package name="14FPC-V">
<description>&lt;b&gt;1mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
<package name="1X14">
</package>
<package name="1X14_LOCK">
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="SOT23-BEC">
<description>&lt;b&gt;TO-236&lt;/b&gt; ITT Intermetall</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="CT3216">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CT3528">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CT6032">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="B45181A">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 5 x 5 mm, rectangle, grid 2.54 mm</description>
</package>
<package name="B45181B">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 7.6 x 5 mm, rectangle, grid 5.08 mm</description>
</package>
<package name="B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="B45181D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.5 x 12.5 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="TT2D4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D4L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="ETR1">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 2.54 mm</description>
</package>
<package name="ETR2">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR3">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="ETR5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="P128-35">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-40">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TAP5-45">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4.5 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-70">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-80">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 8.0 mm, grid 5.08 mm</description>
</package>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="E15-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 6 mm</description>
</package>
<package name="E15-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 9 mm</description>
</package>
<package name="E2,5-4R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="E2,5RE">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm,</description>
</package>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="E22-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 10 mm</description>
</package>
<package name="E22-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 6 mm</description>
</package>
<package name="E22-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="E25-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 10 mm</description>
</package>
<package name="E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="E30-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 10 mm</description>
</package>
<package name="E30-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 12 mm</description>
</package>
<package name="E30-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 35.56 mm, diameter 12 mm</description>
</package>
<package name="E35-14">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 14 mm</description>
</package>
<package name="E35-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 18 mm</description>
</package>
<package name="E45-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 16 mm</description>
</package>
<package name="E45-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 18 mm</description>
</package>
<package name="E45-21">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 21 mm</description>
</package>
<package name="E45-22">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 22 mm</description>
</package>
<package name="E45-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 25 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="E5-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.05 mm, diameter 4 mm</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E50-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 25 mm</description>
</package>
<package name="E50-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 30 mm</description>
</package>
<package name="E55-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 25 mm</description>
</package>
<package name="E55-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 30 mm</description>
</package>
<package name="E5R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 9 mm</description>
</package>
<package name="E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
<package name="E7,5-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 18 mm</description>
</package>
<package name="EB20D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 20 mm</description>
</package>
<package name="EB22,5D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 22.5 mm</description>
</package>
<package name="EB25D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 25 mm</description>
</package>
<package name="EB30D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 30 mm</description>
</package>
<package name="EB35D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 35 mm</description>
</package>
<package name="085CS_1R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AW">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0807">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0808">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 reflow solder&lt;/b&gt;&lt;p&gt;KEMET S / EIA 3216-12</description>
</package>
<package name="A/3216-18W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 reflow solder&lt;/b&gt;&lt;p&gt;KEMET T / EIA 3528-12</description>
</package>
<package name="B/3528-21W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="C/6032-28R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 reflow solder&lt;/b&gt;&lt;p&gt;KEMET U / EIA 6032-15</description>
</package>
<package name="C/6032-28W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wafe solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="D/7343-31R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 reflow solder</description>
</package>
<package name="D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="E/7260-38R">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 reflow solder&lt;/b&gt;</description>
</package>
<package name="E/7260-38W">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Wafe solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12R">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 reflow solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12W">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Wafe solder&lt;/b&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="TT2D5L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_Z">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_P">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SANYO-OSCON_9E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_9F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_A">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_A'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_B">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_B'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_D">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E1">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E9">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F0">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_G">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_H">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_A5">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_B6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_F12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="UD-10X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 10 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-4X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 4 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-5X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 5 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-6,3X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 6.3 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-6,3X7,7_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 6.3 x 7.7 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-8X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 8 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5650</description>
</package>
<package name="C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5664</description>
</package>
<package name="HPC0201">
<description>&lt;b&gt; &lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/10129/hpc0201a.pdf</description>
</package>
<package name="C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
<package name="C1808">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Source: AVX .. aphvc.pdf</description>
</package>
<package name="C3640">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Source: AVX .. aphvc.pdf</description>
</package>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML10L">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="AVR-10PIN-PRG">
</package>
<package name="ML10SMD">
</package>
<package name="1X02">
</package>
<package name="MOLEX-1X2">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X02_BIG">
</package>
<package name="JST-2-SMD-VERT">
</package>
<package name="R_SW_TH">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02_LOCK">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="JST-2-PTH">
</package>
<package name="1X02_XTRA_BIG">
</package>
<package name="1X02_PP_HOLES_ONLY">
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="JST-2-PTH-KIT">
</package>
<package name="1X03">
</package>
<package name="MOLEX-1X3">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="1X03_LOCK">
</package>
<package name="1X03_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X3_LOCK">
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="1X03_LONGPADS">
</package>
<package name="JST-3-PTH">
</package>
<package name="1X03_PP_HOLES_ONLY">
</package>
<package name="SCREWTERMINAL-5MM-3">
</package>
<package name="1X03_LOCK_NO_SILK">
</package>
<package name="JST-3-SMD">
</package>
<package name="1X03-1MM-RA">
</package>
<package name="1X05">
</package>
<package name="1X05-1.27MM">
<description>Header for OS4000-T</description>
</package>
<package name="1X05_LOCK">
</package>
<package name="1X05_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X05_LONGPADS">
</package>
<package name="1X05-1MM">
</package>
<package name="1X05-1MM-RA">
</package>
<package name="HC49">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="HC18-49U">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="TO-46">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
2-lead metall, vertical</description>
</package>
<package name="2X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X07/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="2X16LCDB">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CONTRAST"/>
<pin name="RS" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="E" direction="in"/>
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="LED_A(+5V)" direction="pwr"/>
<pin name="LED_K(GND)" direction="pwr"/>
</symbol>
<symbol name="ATMEGA8">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3" direction="pwr"/>
<pin name="P$4" direction="pwr"/>
<pin name="P$5" direction="pwr"/>
<pin name="P$6" direction="pwr"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20" direction="pwr"/>
<pin name="P$21" direction="pwr"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
</symbol>
<symbol name="MEGA8">
<description>&lt;B&gt;ATMega 8 &lt;/B&gt; (non SMD-version)
&lt;P&gt;
&lt;B&gt;Important features :&lt;/B&gt;&lt;BR&gt;
• &lt;U&gt;Package&lt;/U&gt;&lt;BR&gt;
- 28 PDIP&lt;BR&gt;
• &lt;U&gt;Onboard mems&lt;/U&gt; :&lt;BR&gt;
- 8 KB Flash&lt;BR&gt;
- 1KB SRAM&lt;BR&gt;
- 512 B EEPROM&lt;BR&gt;
• &lt;U&gt;Peripherals :&lt;/U&gt;&lt;BR&gt;
- Two 8-bit Timer / Counters&lt;BR&gt;
- One 16-bit Timer/Counter&lt;BR&gt;
- Six 10-bit ADC&lt;BR&gt;
- Programmable UART&lt;BR&gt;
- RTC with seperate Oscillator&lt;BR&gt;
- Byte oriented 2-wire Serial interface&lt;BR&gt;
- Master / Slave SPI&lt;BR&gt;
- Analog comparator&lt;BR&gt;
• &lt;U&gt;Operating Voltages&lt;/U&gt; :&lt;BR&gt;
- 4.5 - 5.5 V DC (ATMega8)&lt;BR&gt;
- 2.7 - 5.5V DC (ATMega8L)&lt;BR&gt;
• &lt;U&gt;Power Consumption at 4 Mhz, 3V, 25°C&lt;/U&gt; :&lt;BR&gt;
– Active: 3.6 mA&lt;BR&gt;
– Idle Mode: 1.0 mA&lt;BR&gt;
– Power-down Mode: 0.5 μA&lt;BR&gt;
• &lt;U&gt;Speed Grades&lt;/U&gt; :&lt;BR&gt;
– 0 - 8 MHz (ATmega8L)&lt;BR&gt;
– 0 - 16 MHz (ATmega8)</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
</symbol>
<symbol name="RESISTOR">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="PINV">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PIN">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="2X16LCD">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CONTRAST"/>
<pin name="RS" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="E" direction="in"/>
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP-1">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="NPN-1">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CPOL">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ISP-10HEADER">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
</symbol>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="M05">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="XTAL">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="78*SMD">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
</symbol>
<symbol name="LM1117-ADJ">
<pin name="ADJ"/>
<pin name="IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="V-REF">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="PINH2X7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LCD2X16B" prefix="LCD" uservalue="yes">
<description>2x16LCD with backlight (HD44780 compatible)&lt;BR&gt;
Contains 14 pins</description>
<gates>
<gate name="G$1" symbol="2X16LCDB"/>
</gates>
<devices>
<device name="SIL" package="SIL-16">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="P$3"/>
<connect gate="G$1" pin="DB0" pad="P$7"/>
<connect gate="G$1" pin="DB1" pad="P$8"/>
<connect gate="G$1" pin="DB2" pad="P$9"/>
<connect gate="G$1" pin="DB3" pad="P$10"/>
<connect gate="G$1" pin="DB4" pad="P$11"/>
<connect gate="G$1" pin="DB5" pad="P$12"/>
<connect gate="G$1" pin="DB6" pad="P$13"/>
<connect gate="G$1" pin="DB7" pad="P$14"/>
<connect gate="G$1" pin="E" pad="P$6"/>
<connect gate="G$1" pin="GND" pad="P$1"/>
<connect gate="G$1" pin="LED_A(+5V)" pad="P$15"/>
<connect gate="G$1" pin="LED_K(GND)" pad="P$16"/>
<connect gate="G$1" pin="R/W" pad="P$5"/>
<connect gate="G$1" pin="RS" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP" package="2X8">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED_A(+5V)" pad="15"/>
<connect gate="G$1" pin="LED_K(GND)" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-H" package="16FPC-H">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED_A(+5V)" pad="15"/>
<connect gate="G$1" pin="LED_K(GND)" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-V" package="16FPC-V">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED_A(+5V)" pad="15"/>
<connect gate="G$1" pin="LED_K(GND)" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8X-SMD" prefix="IC" uservalue="yes">
<description>&lt;FONT FACE=ARIAL&gt;&lt;B&gt;&lt;FONT COLOR=blue&gt;Atmega 8&lt;/FONT&gt;&lt;/B&gt;&lt;BR&gt;
32-pin microcontroller from ATMEL
&lt;P&gt;
&lt;UL&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;8 KB Flash&lt;/FONT&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;512 B EEPROM&lt;/FONT&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;1 KB SRAM&lt;/FONT&gt;
 &lt;LI&gt;2x 8-bit Timers / Counters
 &lt;LI&gt;1x 16-bit Timer / Counter
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;2x INTs&lt;/FONT&gt;
 &lt;LI&gt;RTC with seperate Oscillator
 &lt;LI&gt;8x 10 bit ADC (TQFP / MLF)
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;23x Programmable I/O lines&lt;/FONT&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;UART&lt;/FONT&gt;
 &lt;LI&gt;Operating Voltage : 4.5 - 5.5 V
 &lt;LI&gt;Speed grade : 0 - 16 MHz
&lt;/LI&gt;
&lt;/UL&gt;
&lt;/P&gt;&lt;/FONT&gt;</description>
<gates>
<gate name="G$1" symbol="ATMEGA8"/>
</gates>
<devices>
<device name="TQFP" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MLF" package="MLF32">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8X-TH" prefix="IC" uservalue="yes">
<description>&lt;FONT FACE=ARIAL&gt;&lt;B&gt;&lt;FONT COLOR=blue&gt;Atmega 8&lt;/FONT&gt;&lt;/B&gt;&lt;BR&gt;
32-pin microcontroller from ATMEL
&lt;P&gt;
&lt;UL&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;8 KB Flash&lt;/FONT&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;512 B EEPROM&lt;/FONT&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;1 KB SRAM&lt;/FONT&gt;
 &lt;LI&gt;2x 8-bit Timers / Counters
 &lt;LI&gt;1x 16-bit Timer / Counter
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;2x INTs&lt;/FONT&gt;
 &lt;LI&gt;RTC with seperate Oscillator
 &lt;LI&gt;8x 10 bit ADC (TQFP / MLF)
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;23x Programmable I/O lines&lt;/FONT&gt;
 &lt;LI&gt;&lt;FONT COLOR=blue&gt;UART&lt;/FONT&gt;
 &lt;LI&gt;Operating Voltage : 4.5 - 5.5 V
 &lt;LI&gt;Speed grade : 0 - 16 MHz
&lt;/LI&gt;
&lt;/UL&gt;
&lt;/P&gt;&lt;/FONT&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA8"/>
</gates>
<devices>
<device name="DIL28" package="DIL28-3">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="TH10" package="0207/10">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="C0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="C0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="C0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH7" package="0207/7">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2VERT" package="0207/2V">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD2X16" prefix="LCD" uservalue="yes">
<description>2x16LCD (HD44780 compatible)&lt;BR&gt;
Contains 14 pins</description>
<gates>
<gate name="G$1" symbol="2X16LCD"/>
</gates>
<devices>
<device name="SMD-H" package="14FPC-H">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-V" package="14FPC-V">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIL14" package="1X14">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIL14-LOCK" package="1X14_LOCK">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X7V" package="2X07">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X7H" package="2X07/90">
<connects>
<connect gate="G$1" pin="CONTRAST" pad="3"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC547*" prefix="T" uservalue="yes">
<description>&lt;b&gt;NPN Transistor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC557*" prefix="T" uservalue="yes">
<description>&lt;b&gt;PNP Transistror&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="TO92-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC857*" prefix="Q">
<description>&lt;b&gt;PNP Transistror&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PNP-1"/>
</gates>
<devices>
<device name="SMD" package="SOT23-BEC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="ALT1"/>
<technology name="B"/>
<technology name="BALT1"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847*" prefix="Q">
<description>NPN Transistor</description>
<gates>
<gate name="G$1" symbol="NPN-1"/>
</gates>
<devices>
<device name="SMD" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="ALT1"/>
<technology name="B"/>
<technology name="BLT1"/>
<technology name="C"/>
<technology name="CLT1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CPOL-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="CPOL"/>
</gates>
<devices>
<device name="CT3216" package="CT3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT3528" package="CT3528">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6032" package="CT6032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT7343" package="CT7343">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181A" package="B45181A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181B" package="B45181B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181C" package="B45181C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181D" package="B45181D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4" package="TT2D4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4L" package="TT2D4L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5" package="TT2D5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6" package="TT2D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6L" package="TT2D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7L" package="TT2D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7" package="TT2D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D10" package="TT5D10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11" package="TT5D11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11L" package="TT5D11L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT6D6" package="TT5D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D6L" package="TT5D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7" package="TT5D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7L" package="TT5D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9" package="TT5D9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9L" package="TT5D9L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR1" package="ETR1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR2" package="ETR2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR3" package="ETR3">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR4" package="ETR4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR5" package="ETR5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-35" package="P128-35">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-40" package="P128-40">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-50" package="P128-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-60" package="P128-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-45" package="TAP5-45">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-50" package="TAP5-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-70" package="TAP5-70">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-60" package="TAP5-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-80" package="TAP5-80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E1.8-4" package="E1,8-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-5AXIAL" package="E15-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-6AXIAL" package="E15-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-9AXIAL" package="E15-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5V" package="E2,5-4R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5" package="E2,5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-6" package="E2,5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-7" package="E2,5-7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-4V" package="E2,5RE">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-4" package="E2-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-5" package="E2-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-10AXIAL" package="E22-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-6AXIAL" package="E22-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-9AXIAL" package="E22-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-10" package="E3,5-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-10AXIAL" package="E25-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-9AXIAL" package="E25-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-8" package="E3,5-8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-10AXIAL" package="E30-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-12AXIAL" package="E30-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-16AXIAL" package="E30-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-12AXIAL" package="E35-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-14AXIAL" package="E35-14">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-16AXIAL" package="E35-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-18AXIAL" package="E35-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-16AXIAL" package="E45-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-18AXIAL" package="E45-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-21AXIAL" package="E45-21">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-22AXIAL" package="E45-22">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-25AXIAL" package="E45-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-10.5" package="E5-10,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-13" package="E5-13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-4" package="E5-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-5" package="E5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-6" package="E5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-8.5" package="E5-8,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-25AXIAL" package="E50-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-30AXIAL" package="E50-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-25AXIAL" package="E55-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-30AXIAL" package="E55-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-9VAXIAL" package="E5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-16" package="E7,5-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-18" package="E7,5-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-20" package="EB20D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-22.5" package="EB22,5D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-25" package="EB25D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-30" package="EB30D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-35" package="EB35D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1R" package="085CS_1R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1W" package="085CS_1W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AR" package="085CS_1AR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AW" package="085CS_1AW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2R" package="139CLL-2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2W" package="139CLL-2W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3R" package="139CLL-3R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3W" package="139CLL-3W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-0810" package="140CLH-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1010" package="140CLH-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1014" package="140CLH-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-0810" package="150CLZ-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1010" package="150CLZ-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1014" package="150CLZ-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0405" package="153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0505" package="153CLV-0505">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0605" package="153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0807" package="153CLV-0807">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0810" package="153CLV-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1010" package="153CLV-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1012" package="153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1014" package="153CLV-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0808" package="175TMP-0808">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0810" package="175TMP-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18R" package="A/3216-18R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18W" package="A/3216-18W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21R" package="B/3528-21R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21W" package="B/3528-21W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28R" package="C/6032-28R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28W" package="C/6032-28W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31R" package="D/7343-31R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31W" package="D/7343-31W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38R" package="E/7260-38R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38W" package="E/7260-38W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12R" package="R/2012-12R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12W" package="R/2012-12W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="PANASONIC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="PANASONIC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F" package="PANASONIC_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5L" package="TT2D5L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2,5-6E" package="E2,5-6E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCA" package="SMC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCZ" package="SMC_Z">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCP" package="SMC_P">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCB" package="SMC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCC" package="SMC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCD" package="SMC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCE" package="SMC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_9E" package="SANYO-OSCON_9E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_9F" package="SANYO-OSCON_9F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_A" package="SANYO-OSCON_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_A'" package="SANYO-OSCON_A'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_B" package="SANYO-OSCON_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_B'" package="SANYO-OSCON_B'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_C" package="SANYO-OSCON_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_C'" package="SANYO-OSCON_C'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_C6" package="SANYO-OSCON_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_D" package="SANYO-OSCON_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E" package="SANYO-OSCON_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E'" package="SANYO-OSCON_E'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E1" package="SANYO-OSCON_E1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E12" package="SANYO-OSCON_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E13" package="SANYO-OSCON_E13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E7" package="SANYO-OSCON_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E9" package="SANYO-OSCON_E9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F" package="SANYO-OSCON_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F'" package="SANYO-OSCON_F'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F0" package="SANYO-OSCON_F0">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F13" package="SANYO-OSCON_F13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F8" package="SANYO-OSCON_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_G" package="SANYO-OSCON_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_H" package="SANYO-OSCON_H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_A5" package="SANYO-OSCON_SMD_A5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_B6" package="SANYO-OSCON_SMD_B6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_C6" package="SANYO-OSCON_SMD_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_E12" package="SANYO-OSCON_SMD_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_E7" package="SANYO-OSCON_SMD_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_F12" package="SANYO-OSCON_SMD_F12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_F8" package="SANYO-OSCON_SMD_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UD-10X10" package="UD-10X10_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UD-4X5,8" package="UD-4X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UD-5X5,8" package="UD-5X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UD-6,3X8,8" package="UD-6,3X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UD-6,3X7,7" package="UD-6,3X7,7_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UD-8X10" package="UD-8X10_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-024X044" package="C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HPC0201" package="HPC0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0201" package="C0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1808" package="C1808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3640" package="C3640">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISP-HEADERS" prefix="ISP" uservalue="yes">
<description>&lt;P&gt;&lt;B&gt;&lt;FONT COLOR='#0000FF'&gt;ISP&lt;/FONT&gt;-programmer header&lt;/B&gt;&lt;BR&gt;
All AVR-microcontroller need to be programmed. You can use JTAG, bootloader or ISP-programming. This library is for ISP-programming, so you need to connect the following pins of an AVR-microcontroller on your PCB :
&lt;UL&gt;
 &lt;LI&gt;MOSI
 &lt;LI&gt;RST
 &lt;LI&gt;SCK
 &lt;LI&gt;MISO
 &lt;LI&gt;GND
 &lt;LI&gt;Vcc (= optional)
&lt;/UL&gt;
&lt;P&gt;&lt;B&gt;&lt;FONT COLOR='#0000FF'&gt;10 pin-&lt;/FONT&gt;version&lt;/B&gt;&lt;BR&gt;
This library contains only 10 pins-female connectors, but are divided into 2 main groups :  &lt;U&gt;SMD-version&lt;/U&gt; and &lt;U&gt;through-hole&lt;/U&gt;. The SMD-version comes in handy, when your PCB lacks space and if you want to avoid some extra drill-holes.
&lt;P&gt;&lt;B&gt;&lt;FONT COLOR='#FF0000'&gt;Note&lt;/B&gt;&lt;/FONT&gt;&lt;BR&gt;
I strongly recommend you not to connect &lt;B&gt;Vcc&lt;/B&gt; if your AVR-microcontroller is already mounted on a PCB which contains it's own powersupply.</description>
<gates>
<gate name="G$1" symbol="ISP-10HEADER"/>
</gates>
<devices>
<device name="10-PINS-UP" package="ML10">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10-PINS-SIDE" package="ML10L">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-10-PINS-SIDE" package="AVR-10PIN-PRG">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10-PINS-SMD" package="ML10SMD">
<connects>
<connect gate="G$1" pin="P$1" pad="P$9"/>
<connect gate="G$1" pin="P$10" pad="P$2"/>
<connect gate="G$1" pin="P$2" pad="P$10"/>
<connect gate="G$1" pin="P$3" pad="P$7"/>
<connect gate="G$1" pin="P$4" pad="P$8"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$3"/>
<connect gate="G$1" pin="P$8" pad="P$4"/>
<connect gate="G$1" pin="P$9" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 2&lt;/b&gt;
Standard 2-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08233 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROCKER" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="1" pad="P$3"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 3&lt;/b&gt;
Standard 3-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X03_NO_SILK" package="1X03_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X03_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-3-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X03_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCREW-5MM" package="SCREWTERMINAL-5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X03_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="JST-3-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X03-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 5&lt;/b&gt;
Standard 5-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08230 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M05"/>
</gates>
<devices>
<device name="PTH" package="1X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X05-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X05_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X05_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X05_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X05-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="1X05-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL" prefix="X" uservalue="yes">
<gates>
<gate name="G$1" symbol="XTAL"/>
</gates>
<devices>
<device name="TH" package="HC18-49U">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="HC49">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V-REG_78*SMD" prefix="IC" uservalue="yes">
<description>&lt;B&gt;Voltage Regulator in SMD&lt;/B&gt;&lt;BR&gt;
This library contains the positive powerregulators of the 78L-familie
&lt;P&gt;
&lt;TABLE CELLSPANNING=0 CELLPADDING=2 BORDER=0&gt;
 &lt;TR BGCOLOR=blue&gt;&lt;TD&gt;&lt;FONT COLOR=white&gt;&lt;B&gt;Specification&lt;/B&gt;&lt;/FONT&gt;&lt;/TD&gt;&lt;TD&gt;&lt;FONT COLOR=white&gt;&lt;B&gt;Value&lt;/B&gt;&lt;/FONT&gt;&lt;/TD&gt;&lt;/TR&gt;
&lt;TR BGCOLOR=lightgrey&gt;&lt;TD&gt;Available versions&lt;/TD&gt;&lt;TD&gt;3.3V / 5.0V / 8.0V / 9.0V / 12.0V&lt;/TD&gt;&lt;/TR&gt;
 &lt;TR&gt;&lt;TD&gt;Output Voltage accuracy&lt;/SUB&gt;&lt;/FONT&gt;&lt;/TD&gt;&lt;TD&gt;+/- 0.25V&lt;/TD&gt;&lt;/TDR&gt;
 &lt;TR BGCOLOR=lightgrey&gt;&lt;TD&gt;Minimum Input Voltage&lt;/SUB&gt;&lt;/FONT&gt;&lt;/TD&gt;&lt;TD&gt;Output Voltage +  3.0 V&lt;/TD&gt;&lt;/TDR&gt;
&lt;TR&gt;&lt;TD&gt;Maximum Current&lt;/TD&gt;&lt;TD&gt;100 mA&lt;/TD&gt;&lt;/TR&gt;
&lt;TR BGCOLOR=lightgrey&gt;&lt;TD&gt;Package&lt;/TD&gt;&lt;TD&gt;SO8&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/P&gt;
&lt;P&gt;
&lt;B&gt;Datasheet&lt;/B&gt;&lt;BR&gt;
A datasheet of i.e. the 5.0V-version, can be found at the following internet-address :&lt;BR&gt;
&lt;FONT COLOR=blue&gt;http://www.alldatasheet.com/view.jsp?Searchword=78L05&lt;/FONT&gt;
&lt;/P&gt;</description>
<gates>
<gate name="G$1" symbol="78*SMD"/>
</gates>
<devices>
<device name="5.0V" package="SO08">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V-REF" prefix="VREF" uservalue="yes">
<description>V-ref diode LM4040</description>
<gates>
<gate name="G$1" symbol="V-REF"/>
</gates>
<devices>
<device name="LM4040" package="SOT23">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LT1004-SO8" package="SO08">
<connects>
<connect gate="G$1" pin="P$1" pad="4"/>
<connect gate="G$1" pin="P$2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LT1004-TO92" package="TO92">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LT1004-TO46" package="TO-46">
<connects>
<connect gate="G$1" pin="P$1" pad="2"/>
<connect gate="G$1" pin="P$2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X7"/>
</gates>
<devices>
<device name="2X7-V" package="2X07">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X7-H" package="2X07/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
