|  |
| --- |
| MAINBOAR  328p top  twi  Rgb led  3  Romote controll / programing  Self programing  ISP  4  Ir Decode  1  Ir Transistor  6  Ir Led  6 |
| MOTORBOARD  Ir Decode (wheel)  2 (3) [4]  rgb sensor  i2c / twi  error Led  1  328p  top  twi  Compass sensor  i2c / twi  ISP  4  Motor driver  4 (5) |
| MOTORBOARD  rgb led  6  328p  buttom  twi  ISP  4  light sensor  4 |